

**TR Switch Schematic rev. 7/29/18** note R10 (1K) should be R11 (1K) To reduce the saturated output from +2.5 dBm to 0 dBm change R9 from 10 to 27 ohms